UPGRADING THE PMU FROM A .combo RELEASE 

1.Flash the .combo image as for any normal OBP release, either from OBP with 
    flash-update or via Solaris using the /usr/Flash system (See /usr/Flash/README). 
2.Reboot the system to ensure the OBP has been upgraded. 
   You may get a message about "NVRAM contents invalid; initializing..." 
   If this happens you will need to do Stop-A to prevent it auto-booting 
   and may want to reset some OBP environment variables: 

   ok setenv diag-switch? false 
   ok setenv auto-boot? false 

3.Turn the system off. 
4.Connect a USB keyboard. If you do not do this and hold down the F key as 
    per (5) the system I/O will go to the serial line and the screen will stay 
    blank. If you can connect the serial line to another machine e.g. using tip 
    it is perfectly ok to proceed with the following steps using the serial line 
    as the console. 
5.Hold down the F key on the main (not USB) keyboard, and reset the system using 
   an unbent paper clip (or similar) in the small reset hole near the centre of 
   on the right hand side of the unit. The 3 leds (Caps, Num & Scr lock) will 
   flash in various ways. 
6.Once the system has started, release the F key. The system should go into an 
   automatic upgrade sequence, update the PMU and then switch itself off. 
   If it does not you can type pmu-update at the ok prompt on the USB kb. 
8.Unplug the USB keyboard and power on the system. 
9.Check that the banner shows the correct PMU revision number. 


